Trimble Inc. Data File Display Program, Version 6.249
Trimble internal use only, not licensed for use outside of Trimble
T01 library 8.154 (BETA 2) - Multicore
Trimble Data File...: 240923_bench/BX992_all.T04


- - - - - - - - - - - - - - - - - - - - - - - - -
Overall file information:

Receiver serial: 6221C43829

First time tag : 2333 151200.000     Last time tag  : 2333 161999.900
First meas tag : 2333 151200.000     Last meas tag  : 2333 161999.800
               : 23Sep2024 18:00:00                 : 23Sep2024 21:00:00

Rec  12:          3
Rec  14:         35
Rec  15:          3
Rec  16:        132
Rec  19:          6
Rec  21:         56
Rec  22:          6
Rec  23:         84
Rec  24:          3
Rec  28:       1248
Rec  30:         12
Rec  31:         45
Rec  32:       2625
Rec  33:         12
Rec  35:     186706
Rec  40:         18
  Total:     190994

Record type 16 subrecords
Sub  27:          3
Sub  37:          3
Sub  43:          3
Sub  44:          3
Sub 124:          9
Sub 199:        111

Record type 28 subrecords
Sub   1:        270
Sub   2:         84
Sub   4:        410
Sub  11:         50
Sub  14:         44
Sub  15:        346
Sub  16:         44

Record type 33 subrecords
Sub   3:          3
Sub  29:          3
Sub  30:          3
Sub  31:          3

Record type 35 subrecords
Sub   2:     108000
Sub   5:          3
Sub   7:          3
Sub  19:      54000
Sub  25:       1080
Sub  28:      10800
Sub  31:      10800
Sub 128:          3
Sub 132:          3
Sub 258:       1080
Sub 259:          3
Sub 262:          3
Sub 267:        180
Sub 268:        180
Sub 270:          9
Sub 272:         19
Sub 273:        540


----- Position Type -----  -Epochs-  -Percent-  -SvsUsed-
              Kalman SBAS    108000      100.0   1337646
                    Total    108000      100.0   1337646

No stored doppler in input file.

Number of t02 file headers detected = 3.
More than one t02 file header can be caused by continuous logging through a power fail, crash, clean reboot, or firmware upgrade. Multiple headers can also be caused by concatenated t02 files.

Errorlog summary (backtrace only stored for current FW):
  total # in flash at startup = 27 (0 with stored backtrace)
  # warnings during runtime = 0
  total # in flash in last record = 27

- - - - - - - - - - - - - - - - - - - - - - - - -
